Additional Modem Information

Video & Sound | Tiberian Sun: Firestorm Support | Install/Uninstall
Error Messages | Modem | Westwood Online
Clans/Tournaments/WDT | IPX Network Play | Other

www.westwood.com

Software Titles

Technical Support

Westwood Online

Online Store

HOME

USR ROBOTICS AND MWAVE MODEMS

US Robotics Sportster Modems

- Click on "Start"
- Click on "Settings"
- Click on "Control Panel"
- Click on "Modem"
- Click on "Properties"
- Click on the "Connection" tab
- Click on the "Advanced" tab
  - Make sure that Use Flow Control is checked, and set to Hardware.
  - Make sure "Error Control" is set to Compress Data.
  - Then, add to the extra settings field S12=0 and S0=4.
    - S0=4: Makes the modem wait for the 4th ring before picking up the call.
    - S12=0: Sets the modem delay to 0.
  - If your US Robotics Sportster Modem is a PnP Modem, then make sure you have removed all the jumpers on the modem board.

MWave SOUND/MODEM CARD:

- IBM Aptivas with MWave modem/sound cards may experience difficulty, especially joining multiplayer games via modem.
- Contact IBM at: www.ibm.com for the latest software update for their MWave DSP which includes support for TAPI and Direct X.

These pages are best viewed with Netscape Navigator or Microsoft Internet Explorer. Windows is a registered trademark of Microsoft Corporation. All right reserved.

© 1999, 2000 Electronic Arts, Inc. All Rights Reserved.